|  |  |
| --- | --- |
| V Set tone type | FW > Mode > dial > mode |
| V Set tone freq | FW > 2 > dial > 2 |
| V Save | FW(1) – Dial – FW [5 sec limit] |
| MR Change name | Menu(1)>#53>Menu>[dial>mode>PTTband to backup, HM/RV(2) clear |
| MR Assign to bank | FW(1) > Dial(B<1) > FW |
| MR to Memory Bank Mode | Band |
| MB Change banks | FW > Band > dial > band |

|  |  |
| --- | --- |
| V Set tone type | FW > Mode > dial > mode |
| V Set tone freq | FW > 2 > dial > 2 |
| V Save | FW(1) – Dial – FW [5 sec limit] |
| MR Change name | Menu(1)>#53>Menu>[dial>mode>PTTband to backup, HM/RV(2) clear |
| MR Assign to bank | FW(1) > Dial(B<1) > FW |
| MR to Memory Bank Mode | Band |
| MB Change banks | FW > Band > dial > band |

|  |  |
| --- | --- |
| V Set tone type | FW > Mode > dial > mode |
| V Set tone freq | FW > 2 > dial > 2 |
| V Save | FW(1) – Dial – FW [5 sec limit] |
| MR Change name | Menu(1)>#53>Menu>[dial>mode>PTTband to backup, HM/RV(2) clear |
| MR Assign to bank | FW(1) > Dial(B<1) > FW |
| MR to Memory Bank Mode | Band |
| MB Change banks | FW > Band > dial > band |

|  |  |
| --- | --- |
| V Set tone type | FW > Mode > dial > mode |
| V Set tone freq | FW > 2 > dial > 2 |
| V Save | FW(1) – Dial – FW [5 sec limit] |
| MR Change name | Menu(1)>#53>Menu>[dial>mode>PTTband to backup, HM/RV(2) clear |
| MR Assign to bank | FW(1) > Dial(B<1) > FW |
| MR to Memory Bank Mode | Band |
| MB Change banks | FW > Band > dial > band |