Band Plans
Band Plans 10 Meters 6 Meters 2 Meters 1.25 Meters 70 Centimeters 33 Centimeters 902.0125 - 902.9875 Repeater Inputs, 12.5 Khz Channels 903.0000 - 905.0000 Digital 910.2500 ATV Repeater Input 915.0000 - 917.0000 Digital 923.2500 ATV Repeater Output 927.0125 - 927.9875 Repeater Outputs, 12.5 Khz channels, -25 Mhz Offset 23 Centimeters 1240.000 - 1246.000 ATV Channel 3, 1241.250 - Video, 1245.750 - Audio 1246.000 - 1248.000 Coordinated Auxiliary links, duplex, 12 Mhz Offset 1248.000 - 1252.000 Digital 1252.000 - 1258.000 ATV Channel 4, 1253.250 - Video, 1257.750 - Audio 1258.000 - 1260.000 Coordinated Auxiliary links, Duplex, 12 Mhz Offset 1264.000 - 1270.000 ATV Channel 5, 1265.250 - Video, 1269.750 - Audio 1270.000 - 1276.000 Repeater Inputs, 25 Khz Channels 1276.000 - 1282.000 ATV Channel 6, 1277.250 - Video, 1281.750 - Audio 1282.000 - 1288.000 Repeater Outputs, 25 Khz Channels, -12Mhz Offset 1288.000 - 1294.000 ATV Channel 7, 1289.250 - Video, 1293.750 - Audio 1294.000 - 1295.000 FM Simplex and Remote Bases 1295.000 - 1297.000 Weak Signal, NO FM in this Sub-Band 1297.000 - 1300.000 Digital Valid Repeater Pairs by Band 10 Meters: 6 Meters: 2 Meters: 1.25 Meters: 70 Centimeters: 33 Centimeters 23 Centimeters © Northern Amateur Relay Council of California, Inc. 2020. All Rights Reserved.